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I. Product Introduction
The Intelligent Security Access Control complies with the ISO18000-6C (EPC C1G2) protocol. It features a sleek and robust design, ensuring stable performance and reliability. This system supports multi-tag reading and utilizes infrared trigger reading mode. It is capable of counting the number of people entering and exiting. The integrated system includes both audio and visual alarms and supports both online and offline EAS alarm modes. The device is equipped with a network port for communication and can be expanded to include Wi-Fi and other communication methods.

II. Product Features
1. Exceptional multi-tag reading capability with extremely low rates of missed and erroneous reads.
2. Specially designed antennas ensure accurate coverage of the access control area without any blind spots.
3. Built-in alarm lights and buzzers.
4. The RFID security gate can be placed at a wider distance, with a maximum distance of up to 3 meters.
5. External display can be connected to show real-time information and quantities of items passing through, as well as to count the number of people entering and exiting.

III. Specification Parameters

	Main Specification Parameters

	Product Model
	[bookmark: _GoBack]RIA10

	Performance Parameter

	Operating System
	Custom System

	Identification Method
	UHF RFID

	Read/Write Function
	Supports multi-tag identification, tag data filtering, and RSSI signal strength sensing

	Reading Distance
	0-300cm (optimal within 1.2 meters for personnel access control)

	Function
	Audio-visual alarm/Infrared trigger

	Physical Parameters

	Dimensions (HWD)
	1565mm*400mm*120mm


	Communication Interface
	Ethernet, Wi-Fi, RS232

	Installation Method
	Comes with connection cables and power adapter. Easy installation

	UHF RFID

	Frequency Range
	840MHz-960MHz

	RF Protocol Standard
	ISO 18000—6C( EPC C1 G2)

	Power

	Power Supply
	Use the included power adapter

	Operating Environment

	Working Temperature
	0~60℃

	Working Humidity
	10%RH~90%RH
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IV. Product Dimensions
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400mm 34mm

High 1565mm
Wide  400mm

Thickness  34mm Weight  19Kg

Basesize  340x120x222mm  Voltage  110-220V AC

Colour Black - White
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