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I. Product Introduction
The dual-frequency anti-theft system supports both 58 kHz AM anti-theft detection and 900 MHz RFID anti-theft detection. The RFID frequency band complies with the ISO 18000-6C (EPC C1G2) standard, featuring a sleek and sophisticated design with stable quality and reliable performance. It supports multi-tag reading, employs radar-triggered reading mode, enables entry/exit count statistics, and integrates audio-visual alarms. The device supports network interface communication and can be expanded with various communication protocols such as Wi-Fi.
II. Product Features
1. RFID tags possess exceptional reading capabilities with an extremely low missed-read and mis-read rate.
2. The  antenna  is  specially  designed  
3. Built-in alarm light and buzzer
4. The RFID security door is installed at a wider spacing, with a maximum distance of 3 meters.
5. Supports external display for real-time display of item information and quantities, with capability to track entry and exit counts.


III. Specifications and Parameters

	Main specification parameters

	product model
	RIA20

	Performance Parameter

	operating system
	custom-built system

	Identification Method
	Radio Frequency Identification (UHF RFID)

	Reading and Writing Functions
	Supports multi-tag recognition, tag data filtering, and RSSI (received signal strength indicator) measurement

	Installation distance
	1.8m

	Alarming Method
	Color LED lights, buzzer (audio-visual alarm)

	Support tag frequency
	Either AM or UHF RFID; or a dual-frequency system combining AM and UHF RFID.

	Physical Parameter

	Overall dimensions (height * width * depth)
	1510mm*330mm*130mm

	packing measurement
	1640mm*420mm*250mm

	Weight after packaging
	40kg

	CI
	AM: Wireless Wi-Fi, supports remote debugging; RFID: Ethernet port, Wi-Fi, RS232

	way to install
	The kit includes connecting cables and a power adapter. Installation is simple.

	Frequency

	RFID service frequency
	840MHz-960MHz

	Radio Frequency Protocol Standards
	ISO 18000—6C( EPC C1 G2)

	AM service frequency
	58KHZ

	RFID UHF antenna
	8dBi narrow-beam antenna

	Source

	Power Supply Input
	220V/110V AC available as an option.

	Operational Environment

	working temperature
	0~60℃

	Working humidity
	[bookmark: _GoBack]10%RH~90%RH
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