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一、  Product Introduction


[bookmark: _GoBack]The embedded RFID sensing frame is mainly used for batch RFID tag reading in unattended supermarkets and unmanned warehouses. When goods are sold or collected, the RFID sensing frame quickly scans tags to identify item information for sales or requisition.
By connecting an external display screen to the embedded RFID sensing frame, sales data can be updated, payment information displayed, and the anti‑theft bits of commodity tags rewritten. Customers can make batch checkout for purchased items.

二、  Product Features


Adopts a specially designed identification frame structure to improve recognition efficiency, capable of identifying more than 30 items at a single time.
Features an optimized dedicated antenna design, limiting peripheral cross‑reading within 20 cm to effectively solve cross‑reading and missed‑reading problems.
Supports human‑computer interaction via an external display screen and data transmission through an Ethernet port.
Integrated design with a stylish appearance, human‑friendly operation interface and workflow for simple and convenient operation.
Supports embedded installation according to actual site conditions.



三、  Technical Specifications

	Main Specifications

	Product Model
	RCD003

	Performance Parameters

	Identification Method
	Radio Frequency Identification (UHF RFID)

	Frequency Range
	840MHz-960MHz

	RF Protocol Standard
	ISO 18000-6C（EPC C1 G2）

	Reading Time
	3‑5 seconds

	Recognition Quantity
	≥30 items



	Physical Parameters

	Overall Dimensions (L×W×D)
	572mm*492mm*295.5mm

	Communication Interface
	Serial Port

	Power Supply

	Input Voltage
	DC 12V/4A

	Operating Environment

	Operating Temperature
	-10℃~60℃

	Operating Humidity
	10%RH~90%RH



四、  Product Appearance


l Starry Black + Matte White + White Blister Frame
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l Starry Black + Champagne Gold + White Blister Frame
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l Starry Black + Starry Black + White Blister Frame
[image: ]


[image: ]

[image: ]

image2.png




image3.png




image4.png




image5.png




image6.png




image7.jpeg




image1.jpeg




